{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Form for the computation of the minimum and maximum scattering angle"]
[]
[null,"additional camera segments",0]
[]
[null,"camera length",0.5,"m"]
[]
[null,"beam stop diameter",4,"mm"]
[null,"max. usable detector length",0.15,"m"]
[null,"Energy",11,"keV"]
[]
[{"$nulls":7},"   "]
[]
[null,"wavelength",1.127269776415844,"A"]
[]
[]
[null,"theta max",0.14572839723893355,"radians"]
[null,"theta min",0.0019999893334357323,"radians"]
[]
[]
[null,"qmax",1.6189902724163163,"1/A"]
[null,"qmin",0.02229798909847285,"1/A"]
[]
[]
[null,"(1/d)max",0.2576368988568295,"1/A"]
[null,"(1/d)min",0.003548375095237564,"1/A"]
[]
[]
[null,"dmin",3.881431597869475,"A"]
[null,"dmax",281.8191350012984,"A"]
[]
[]
[null,"max. Rg",22.423546706023107,"A"]
[null,null,"qmin x Rg <0.5"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}