{"text_format":"5","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"props":{"creator":"Melissa Mabie-Havlisch","last_modified_by":"Turner User","company":"The Turner Corporation"},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":2,"rows_kept":42,"headers":{"header":["","Turner / LCLS Chemical Proposed Use"]},"flags":["formulas_cached_only"]}
["Contractor"]
[null,"Chemical Trade Name"]
[]
["A & B Construction"]
[null,"314 Liquid Epoxy"]
[null,"SIKATOP 123 Plus-Part A"]
[]
[]
["Affholder, Inc."]
[null,"4000 PSI Granite Rock Concrete"]
[null,"Integral Waterpeller (Dry)"]
[null,"St-Alkali Free Liquid Accelerator"]
[null,"MEYCO® SA 160"]
[null,"FORTA FERRO® "]
[null,"QUICKCRETE Dry Packaged "]
[null,"Micorsiilca EMS 965; EMS 970 DA; microlite-P; EMS-960"]
[null,"Crushed stone, Sand gravel"]
[null,"Burke Plug"]
[]
["Conco"]
[null,"Adeka Ultra Seal® MC"]
[]
["Cupertino Electric"]
[null,"Weld-On Duit 2400"]
[null,"Gorilla PVC Cement"]
[null,"Cantex #99 "]
[null,"Marking paint"]
["OC McDonald"]
[]
["Top Grade"]
[null,"Weld-On 1007"]
[null,"Weld-On 4007"]
[null,"White Cap Creteaway"]
["Western Maintenance"]
[null,"WD-40"]
[null,"Pressure Treated Wood"]
[null,"Unleaded Gasoline"]
[null,"Spray Paint"]
[]
["Jacobs"]
[null,"MELMENT F10"]
[null,"Cement"]